(PIN-001 STANDARD PROGRAM)

N1 G21 T0100				Metric units and Tool 1 - no wear offset
N2 G96 S100 M03				CSS at 100 m/min - CW spindle rotation
N3 G00 X53.0 Z0 T0101 M08		Start position for face cut + wear offset + coolant
N4 G01 X-1.8 F0.1			Face just below centerline at 0.1 mm/rev feedrate
N5 G00 Z3.0				Clear-off face - Z-axis only - by 3 mm
N6 G42 X51.0				X-start for G71 cycle and tool radius offset
N7 G71 U2.5 R1.0			G71 - 2.5 mm cutting depth, 1.0 retract
N8 G71 P9 Q14 U1.5 W0.125 F0.3		G71 - N9 to N14 contour - XZ stock - 0.3 mm/rev
N9 G00 X16.0				Calculated X-diameter for chamfer
N10 G01 X24.0 Z-1.0 F0.1		Cut front chamfer at 0.1 mm/rev
N11 Z-23.0 R3.0 F0.15			Cut small diameter + inner radius at 0.15 mm/rev
N12 X46.0 R-2.0				Cut face and outer radius
N13 Z-47.0				Cut large diameter 3 mm past part length
N14 X54.0 F0.3				Clear-off stock diameter - X-axis only - by 2 mm
N15 G70 P9 Q14 S125			G70 Finish contour at 125 m/min
N16 G00 G40 X100.0 Z50.0 T0100 M09	Rapid to tool change position + cancellations
N17 M01					Program stop (optionally - next tool expected)
